Apple Scribe Printer: Configuration Table
System SW-1 Cable Required
12345678
--------------------------------------------
Apple III 11010000 A+B
Macintosh 11010000 C
Lisa 11010000 A+B
Apple IIc 11010000 E *
Super Serial 11010000 B
High Speed Serial N/A N/A

Key: 0 = off = open; 1 = on = closed
* - Using default port settings

Cables: Letter Part Number Comments

A 590-0029-00 Modem Eliminator
B 590-0037-B DB-25 to DB-25
C 590-0169 DB-9 to DB 25
E 590-0191-A 5-pin DIN to DB-25

Apple III Driver Configuration:

Driver Data Configuration Block

0 1 2 3 4 5 6 7 8 9 A B
RS-232 0E 00 10 10 10 00 13 11 DF 84 50 80
Printer 0E 00 10 10 10

Super Serial Card Configuration:

1 2 3 4 5 6 7
SW1 Off Off Off On Off On On
SW2 On On Off Off On Off Off

The jumper block should be pointing towards terminal.